Gathering Valve Naming

Regular valves are signified by V and Emergency Valves by EV.  Start at the beginning of the line with either V or EV and work your way toward the end of the line with a sequence similar to below.

EV-100, V-200, V-300, EV-400

For blowdowns on either side of the block valve use the identifiers such as for *V-200 (main line block valve) use:*

*V-200-U (upstream blowdown valve)*

*V-200-D (downstream blowdown valve)*

*V-200-B (bypass valve in the crossover)*